Page 1 / 50

SOHO CDS

Operations Manual

Editor: Eddie Breeveld

MSSL/UCL

Document `ID´

Issue 0.2, 18 Aug 1995

Contents

1. Introduction (KN/PDT) ................................ ................................ ................................ ..... Error! Bookmark not defined.

1.1. Revisions ................................ ................................ ................................ ............ 6

1.2. Distribution and Intended Users ................................ ................................ ......... 6

1.3. Reference Documents ................................ ................................ ......................... 6

1.4. Summary and Purpose of Document ................................ ................................ .. 6

2. Instrument Description (DJP/ECS) ................................ ................................ ................... Error! Bookmark not defined.

2.1. CDS Mechanical and Optical Details - ECS ................................ ...................... 2

2.1.1. Mechanical Design ................................ ................................ .............. 2

2.1.2. Optical Design ................................ ................................ ..................... 2

2.1.3. Mechanisms ................................ ................................ ......................... 2

2.1.4. Thermal Control System ................................ ................................ ...... 2

2.2. CDS Electrical Architechture ................................ ................................ ............. 2

2.2.1. Electrical block dia - Alecs Pic ................................ ............................ 2

2.2.2. Power Switching ................................ ................................ .................. 2

2.2.3. Redundancy - SCIF, IMIF, Science interfaces, power ......................... 2

2.3. Operational Concepts ................................ ................................ ......................... 2

2.3.1. CDS Modes ................................ ................................ .......................... 2

2.3.2. Observing Sequences ................................ ................................ ........... 2

2.3.3. Instrument Health Monitoring ................................ ............................. 2

2.4. CDS Commanding and Control ................................ ................................ ......... 2

2.4.1. Introduction ................................ ................................ .......................... 2

2.4.2. Types of Command ................................ ................................ .............. 2

2.4.3. Commandable Subsystems ................................ ................................ .. 2

2.4.4. CDHS Tables ................................ ................................ ....................... 2

2.4.5. CDHS Contol ................................ ................................ ....................... 2

3. Instrument Work Station (JP) ................................ ................................ ............................ 2

Page 2 / 50

3.1. Configuration ................................ ................................ ................................ ..... 2

3.1.1. What needs to be done (in words) ................................ ....................... 2

3.1.2. How to do it (which buttons to press etc) ................................ ............ 2

3.2. Start Up Procedure ................................ ................................ ............................. 2

3.2.1. What ................................ ................................ ................................ ..... 2

3.2.2. How ................................ ................................ ................................ ..... 2

3.3. Commands ................................ ................................ ................................ .......... 2

3.3.1. What ................................ ................................ ................................ ..... 2

3.3.2. How ................................ ................................ ................................ ..... 2

3.4. Databases ................................ ................................ ................................ ............ 2

3.4.1. What ................................ ................................ ................................ ..... 2

3.4.2. How ................................ ................................ ................................ ..... 2

3.5. Playback ................................ ................................ ................................ ............. 2

3.5.1. What ................................ ................................ ................................ ..... 2

3.5.2. How ................................ ................................ ................................ ..... 2

3.6. Data Monitor ................................ ................................ ................................ ...... 2

3.6.1. What ................................ ................................ ................................ ..... 2

3.6.2. How ................................ ................................ ................................ ..... 2

3.7. Engineering Monitor (EMON) ................................ ................................ ........... 2

3.7.1. Detail any standard daily tasks where EMON is to be

used. ................................ ................................ ................................ ............... 3

3.7.2. Explain about EngA/B packets in science stream. .............................. 3

3.7.3. How to find out what they contain. ................................ ..................... 3

3.7.4. Brief overview of what EMON can be used for. ................................ . 3

3.7.5. Packaging EMON to perform specific tasks. ................................ ....... 3

3.7.6. Error monitoring (EMON_ERROR) ................................ ................... 3

4. Observation Planning (CDP) ................................ ................................ ............................. 3

4.1. Overview of planning ................................ ................................ ......................... Error! Bookmark not defined.

4.1.1. Philosophy of planning in view of need for non-RT

observations. ................................ ................................ ................................ .. 11

4.1.2. Resume of how observations are controlled on board

(deferred command list, sequence tables, raster tables etc.) .......................... 11

4.1.3. Resume of how complete planning process is supposed

to work. ................................ ................................ ................................ .......... 11

4.2. Planning databases and access to them ................................ .............................. 11

4.2.1. Resume of database use (why use them). ................................ ............ 12

4.2.2. Explain distinction between private and project

databases. ................................ ................................ ................................ ....... 12

4.2.3. Define controls to be exercised over each of them. ............................. 12

4.2.4. Resume of routines to interact with them (’show’

routines). ................................ ................................ ................................ ........ 12

4.3. Technical planning (mk_raster) ................................ ................................ .......... 12

4.3.1. Review of what it’s for, what it does. ................................ .................. 12

4.3.2. Mention on-line help. ................................ ................................ .......... 12

4.4. Science planning ................................ ................................ ................................ 12

4.4.1. mk_study, why and briefly how to use it. ................................ ............ 12

4.4.2. mk_detail, ditto ................................ ................................ .................... 12

4.4.3. mk_plan ditto ................................ ................................ ....................... 12

Page 3 / 50

4.5. Command preparation (CPT) ................................ ................................ ............. 12

4.5.1. Review of use. ................................ ................................ ..................... 12

4.6. Uplinking commands via Perl scripts ................................ ................................ . 12

4.7. Real time operations. ................................ ................................ .......................... 12

4.7.1. What you can and can’t do ................................ ................................ ... 12

4.8. Deferred Commands ................................ ................................ .......................... 12

4.8.1. What ................................ ................................ ................................ ..... 13

4.8.2. How ................................ ................................ ................................ ..... 13

5. Data Processing (CDP) ................................ ................................ ................................ ...... 13

5.1. Explain about science stream and what’s in it. ................................ ................... 13

5.2. Mention tm files and refer to section ?? of OM for details. ............................... 13

5.3. Overview of science telemetry monitor (STM) ................................ .................. 13

5.3.1. Who can use it. ................................ ................................ .................... 13

5.3.2. What it can/cannot do (briefly) ................................ ............................ 13

5.4. FITS files ................................ ................................ ................................ ............ 13

5.4.1. What are they? ................................ ................................ ..................... 13

5.4.2. How to start generation program. ................................ ........................ 13

5.4.3. How to check things are working OK ................................ ................. 13

5.4.4. How to read a FITS file and display data in IDL ................................ . 13

5.4.5. Use of QL programs. ................................ ................................ ........... 13

5.5. Archives ................................ ................................ ................................ ............. 13

5.5.1. Overview of what they will contain ................................ ..................... 13

5.5.2. How will they be created? ................................ ................................ ... 13

5.5.3. How to access them. ................................ ................................ ............ 13

5.5.4. Distribution of archive CDS data. ................................ ....................... 14

6. Basic Functions (DJP) ................................ ................................ ................................ ....... 14

6.1. Emergency Procedures ................................ ................................ ....................... 14

6.2. CDS Switch On and Off ................................ ................................ ..................... 14

6.2.1. Power Configuration ................................ ................................ ............ 14

6.2.2. CDHS Configuration ................................ ................................ ........... 14

6.3. Power-Up Defaults ................................ ................................ ............................. 14

6.3.1. Default Mode ................................ ................................ ....................... 14

6.3.2. Default CDHS Table contents ................................ ............................. 14

6.3.3. Default Software Status ................................ ................................ ....... 14

6.4. Thermal Control ................................ ................................ ................................ . 14

6.4.1. Non-Operational Heaters (Spacecraft Controlled) .............................. 14

6.4.2. Operational Heaters ................................ ................................ ............. 14

6.5. Modifications to Default Configuration ................................ ............................. 14

6.5.1. Mode Tables ................................ ................................ ........................ 14

6.5.2. System Sequences ................................ ................................ ................ 14

6.5.3. Redundant hardware ................................ ................................ ............ 14

6.6. System Preparation for Science Observations ................................ .................... 15

6.6.1. Secondary Processor ................................ ................................ ............ 15

6.6.2. Optional CDHS Software Modules ................................ ..................... 15

6.6.3. Cleaning Up Telemetry Displays ................................ ......................... 15

6.6.4. Pointing ................................ ................................ ................................ 15

6.6.5. CDS Physical Pointing ................................ ................................ ........ 15

Page 4 / 50

6.6.6. Pointing Software ................................ ................................ ................ 15

6.6.7. Mode Transitions ................................ ................................ ................. 15

6.7. Uploading Observing Sequences ................................ ................................ ........ 15

6.7.1. Uploads ................................ ................................ ................................ 15

6.7.2. Upload Validation ................................ ................................ ................ 15

6.8. Recovery From a Cocked Up Situation ................................ .............................. 15

7. Scientific Operations (ERB) ................................ ................................ .............................. 15

7.1. GIS Operation ................................ ................................ ................................ ..... 15

7.1.1. Pre-operational Checks ................................ ................................ ........ 15

7.1.2. Uploading Tables ................................ ................................ ................. 16

7.1.3. Selecting and Running Observation Sequences ................................ .. 16

7.1.4. Complete Example ................................ ................................ .............. 16

7.2. VDS Operation ................................ ................................ ................................ ... 16

7.2.1. Pre-operational Checks ................................ ................................ ........ 16

7.2.2. Uploading Tables ................................ ................................ ................. 16

7.2.3. Selecting and Running Observation Sequences ................................ .. 16

7.2.4. Complete Example ................................ ................................ .............. 17

7.3. Combined Operations ................................ ................................ ......................... 17

7.3.1. Configuration Commands ................................ ................................ .... 17

7.3.2. Upload and Enable ................................ ................................ ............... 17

7.4. CDS Pointing ................................ ................................ ................................ ..... 17

7.4.1. Commands ................................ ................................ ........................... 17

7.4.2. Inter-Instrument Data Exchange ................................ .......................... 17

7.5. Running and Monitoring Observing Sequences ................................ ................. 17

7.5.1. Realtime - with Ground Contact ................................ .......................... 17

7.5.2. Playback - Out of Ground Contact ................................ ...................... 18

7.6. Recovery from Cocked-Up Situation ................................ ................................ . 18

7.6.1. Panic ................................ ................................ ................................ .... 18

7.6.2. Fix it - don’t call me ! ................................ ................................ ........... 18

7.7. Calibration ................................ ................................ ................................ .......... 18

7.7.1. What ................................ ................................ ................................ ..... 18

7.7.2. How ................................ ................................ ................................ ..... 18

8. Detailed GIS Procedures (ERB/AAB) ................................ ................................ .............. 18

8.1. Four Types of data ................................ ................................ .............................. 18

8.1.1. Raw data with UV ................................ ................................ ............... 18

8.1.2. Science Data with UV ................................ ................................ ......... 19

8.1.3. Filament Data ................................ ................................ ...................... 19

8.2. Obtaining the best science data ................................ ................................ .......... 20

8.3. Corrections to the FITs science data ................................ ................................ .. 24

8.3.1. Electronic Dead times ................................ ................................ .......... 24

8.3.2. Gain Depression ................................ ................................ .................. 26

8.3.3. Background ................................ ................................ .......................... 27

8.3.4. Ghosts ................................ ................................ ................................ .. 28

8.3.5. LUT corrections ................................ ................................ ................... 28

8.3.6. Intensity Curves ................................ ................................ ................... 29

8.3.7. Wavelength Corrections ................................ ................................ ...... 29

8.4. Calibration ................................ ................................ ................................ .......... 30

Page 5 / 50

8.4.1. What ................................ ................................ ................................ ..... 30

8.4.2. How ................................ ................................ ................................ ..... 30

8.5. Obtaining Science Data and Using the Science Analyser ................................ .. 30

8.5.1. What ................................ ................................ ................................ ..... 30

8.5.2. How ................................ ................................ ................................ ..... 31

9. Detailed VDS Procedures (WTT) ................................ ................................ ..................... 31

9.1. What ................................ ................................ ................................ ................... 31

9.2. How ................................ ................................ ................................ .................... 31

10. Engineering Activities (ECS) ................................ ................................ .......................... 31

10.1. Mechanism Maintenance ................................ ................................ .................. 31

10.1.1. What ................................ ................................ ................................ ... 31

10.1.2. How ................................ ................................ ................................ ... 31

10.2. Mechanism Monitoring ................................ ................................ .................... 31

10.3. Relay Monitoring ................................ ................................ ............................. 31

10.4. VDS Exposure Monitoring ................................ ................................ ............... 31

10.5. Thermal Monitoring ................................ ................................ ......................... 31

10.6. Thermal Adjustment ................................ ................................ ......................... 31

10.7. Contamination Monitoring ................................ ................................ ............... 31

11. Appendices ................................ ................................ ................................ ...................... 31

11.1. Command List ................................ ................................ ................................ .. 32

11.1.1. What ................................ ................................ ................................ ... 32

11.1.2. How ................................ ................................ ................................ ... 32

11.2. Telemetry Parameters ................................ ................................ ....................... 32

11.2.1. What ................................ ................................ ................................ ... 32

11.2.2. How ................................ ................................ ................................ ... 32

11.3. And all other IWS databases ... ................................ ................................ ........ 32

11.3.1. What ................................ ................................ ................................ ... 32

11.3.2. How ................................ ................................ ................................ ... 32

Additional Information:

This book will replace the current version of the `Green Book´. Richard and I will

have to ensure that information already in the Green Book, but not mentioned below,

is transferred to the `Blue Book´.

Detailed sub-headings are required from each author by 25 April. These will then be

discussed by the Green Book panel at MSSL, as well as at RAL, before actual inputs

are required.

I have added more subheadings to each item, to try and produce a consistent style for

the whole document. Please follow these suggestions if possible.

Page 6 / 50

1. Introduction (KN/PDT)

1. 1 Revisions

Issue Date Who Comments

0.0 First Release

1. 2 Distribution and Intended Users

1. 3 Reference Documents

1. 4 Summary and Purpose of Document

2. Instrument Description (DJP/ECS)

2. 1 Optical and Mechanical Details

2. 1 .1 Optical design

Fig 2.1.1.1 shows the optical elements of CDS. The telescope focuses an image of

part of the sun onto the slit after a reflection of off the scan mirror. This image can be

viewed by either the normal incidence spectrometer (NIS) or the grazing incidence

spectrometer (GIS).

The telescope aperture is divided into two, one for each of the spectrometers. Light

from the upper aperture passes through the slit and falls onto a pair of toroidal gratings

at near normal incidence which focus dispersed spectra back onto a two dimensional

detector called the viewfinder detector system or VDS. The gratings are inclined

relative to one another such that two spectra fall onto the VDS detector, one above the

other. This spectrometer is stigmatic and uses a long thin slit.

Light from the lower aperture passes through the slit and hits a spherical grating at

grazing incidence and is then dispersed to four, one dimensional detectors spaced

around the Rowland Circle. This spectrometer is astigmatic and uses a pinhole.

Images can be built up by using either the NIS and scanning the scan mirror, or by

using the GIS and moving the pinhole and slit in a raster pattern.

The useful field of view of the telescope is 4 arc mins, to cover the whole solar disc

and the lower corona the whole instrument can be pointed through an angle of +/- 0.75

degrees.

Page 7 / 50

Optical Characteristics of CDS

The telescope Outer f-number

Eff Focal Length

FWHM

Full Geometric Area

Plate Scale at Slit

9.38

257.831 cm

<2 arcsec

289.28cm 2

12.5μm/arcsec

NIS Telescope Aperture Used

Wavelength Ranges

Prime Slits

Grating Ruling

Slit-Grating Dist

Grating-Detector Dist

34.3cm 2 per grating

308 - 381, 513 - 633 Å

2 x 240.4 x 240.90 x 240 arcsec

2400 & 4000 lines/mm

736.5mm

744.6mm

GIS Telescope Aperture Used

Wavelength Ranges

Prime Slits

Grating Ruling

Rowland Circle Radius

47cm 2

151 - 221, 256 - 338,

393 - 493, 656 - 785 Å

2 x 2, 4 x 4, 8 x 50 arcsec

1000 lines/mm

750mm

2. 1 .2 Mechanical Design

All the optical components with the exception of the telescope are housed in an

enclosed spectrometer for reasons of contamination control, ease of alignment and

stray light rejection, see Fig 2.1.2.1. The spectrometer and telescope are mounted in

an outer structure consisting of an aluminium alloy framework see Figs 2.1.2.2 & 3.

In front of the telescope is the +Z panel which carries the two aperture doors.

The mechanism control electronics together with electronics to service the detector

systems are mounted on a platform above the optics bench.

The instrument is mounted on the spacecraft by means of six ball jointed legs, the rear

two being linear actuators which allow the necessary pointing.

Page 8 / 50

2. 1 .3 Mechanisms

2. 1 .3 .1 Aperture door mechanisms

To minimise contamination to the telescope, doors are fitted over both the telescope

apertures. These will be closed on launch and opened some time into the mission.

After that they can be closed as necessary to avoid contamination during attitude

control manoeuvres when the spacecraft thrusters are fired.

The doors are a very simple design. A magnetic latch holds the door closed against a

torsion spring. On command a current is passed through a coil around the permanent

magnet cancelling the magnetic field allowing the torsion spring to open the door.

There are two coils around the magnet for redundancy, one can be controlled by CDS

the other by direct spacecraft command. Under normal circumstances the coil

operated by CDS will be used, in which case current is applied for a limited time

(approximately half a second). In the unlikely event of CDS not being able to open

one or both doors by command, a direct spacecraft command will be used to open

both doors simultaneously. Commands of this type operate relays, consequently the

power would continue to be applied to the coils for some time. To prevent this

occurring, the doors operate microswitches as they open cutting off the power to the

coils.

Stepper motors are fitted to end of each shaft which allow the doors to be closed

independently by command. Magnetic reed switches indicate door open and door

closed position for each door.

2. 1 .3 .2 Scan mirror mechanism

The NIS is a stigmatic instrument which uses a long slit. To build up two dimensional

pictures, images of the Sun are scanned across the entrance slit, in an east/west or

west/east direction by the scan mirror. The scan mirror is mounted in a housing which

is supported by a pair of Bendix flex pivots which allow a few degrees of movement.

An arm projects out the back of the housing which can be moved by a recirculating

ball screw and carriage arrangement to give the necessary angular movement of the

mirror and housing. The ballscrew is rotated by a size 13, 200 per rev stepper motor.

An absolute optical shaft angle encoder tells the operator unambiguously which step

position the motor is at any time. The operating range of the motor is less than one

revolution so no full rev indicator is required. Micro switches are fitted to ensure that

the carriage does not hit the end stops in the event of a software error.

2. 1 .3 .3 Scan mirror mechanism parameters

Operating Steps +/- 64 Steps

Raster step size 2.032 arc sec

Raster range +/- 130 arc sec

Mirror home position Zero

Step rate 30 Hz

Page 9 / 50

2. 1 .3 .4 Slit drive mechanism

The GIS is an astigmatic instrument and builds up images by scanning a pin hole in a

north/south or south/north direction combined with movements of the scan mirror.

The slit drive mechanism consists of a 200 step size 13 stepper motor driving a 0.1

inch pitch, recirculating ball screw which is attached to a carriage supported by a pair

of cross roller slideways. There are six slits attached to the slideway, their centres

being spaced 0.2 inches apart which is two rotations of the ball screw. A coarse linear

encoder consisting of an array of LEDs and photodiodes indicated which slit is in the

line of sight (slit number) and an optical shaft angle encoder attached to the motor

shaft indicates the position of the selected slit (slit position). The linear encoder

incorporates limits to prevent accidental operation outside the normal operating range.

2. 1 .3 .5 Slit number parameters

Slit number Slit size arc sec Slit size mm

1 2 x 2 2 5 μ m x 2 5 μ m

2 4 x 4 5 0 μ m x 5 0 μ m

3 8 x 50 100μm x 0.625mm

4 2 x 240 25μm x 3mm

5 4 x 240 50μm x 3mm

6 90 x 240 125mm x 3mm

Motor step size 1.016 arc sec 12.7μm

Slit home position 00

Slit range slit 1 +/- 120 steps

slit 2 +/- 118 steps

slit 3 +/- 95 steps

slit 4 - 6 zero

Step rate 30Hz

Page 10 / 50

2. 1 .3 .6 Offset pointing mechanism

The CDS instrument is attached to the spacecraft by six ball jointed legs. The rear

two legs are linear actuators which allow the whole instrument to be pointed through

an angle of approximately +/- 0.75 degrees to cover the whole solar disc, a significant

portion of the corona and to allow for some misalignment of the instrument relative to

the spacecraft. The actuators consist of 200 step, size 23 hollow shaft stepper motors,

driving a plain nut and screw assembly of 1mm pitch. Position readout is provided by

a redundant pair of hybrid track potentiometers.

The step increments and the potentiometer digitisation do not match one to one. 5000

motor steps are digitised into 4096 increments by the encoder, consequently one

motor step is 1.22 encoder increments.

The drive system incorporates software end stops in addition to microswitches which

limit movement in the case of a software error. The actuators are inclined at 45

degrees to the spacecraft platform and to the north/south axis of the Sun. This causes

a pointing envelope as shown below.

45´ 15´

32´

2. 1 .3 .7 Offset pointing mechanism parameters

Home position 80, 80

2. 1 .3 .7 .1 Pointing range set by software end stops

encoder readings + 1536 to - 1536

angular position +/- 45 arc min

Position of Microswitch end stops LH: + 1620, - 1640

RH: + 1603, - 1672

Motor step size 0.005mm, approx 1 arc sec

Step rate 14 Hz fixed

Page 11 / 50

2. 1 .4 Thermal Design

The thermal design of CDS comprises both active and passive components. The

temperature of the structure and optics bench are maintained at 20 degrees with a

maximum gradient of 2 degrees.

There is 19 watts of solar energy entering CDS1 through the telescope apertures, half

of which is absorbed by the gold coated mirrors and radiated back through the

apertures to space or conducted through the support to the front bulkhead. From here

it is conducted along the forebody and radiated to space through the telescope radiator,

an exposed part of the forebody that has a good view to space. The solar energy that

is not trapped by the telescope continues into the optics bench where it encounters the

first thermal stop which absorbs unwanted components of the beam and thus reduces

the flux onto the scan mirror. The scan mirror and its mount absorb up to one watt

and reflect the rest onto the second thermal stop which absorbs the remaining

unnecessary components of the beam and admits to the slit only about 0.2 watts. Both

thermal stops are conductively coupled to a radiator on the side of the instrument.

The VDS CCD is required to operate below -80 degrees. To achieve this it is

conductively coupled to a large radiator on the top of the instrument that radiates

directly to space.

With the exception of the radiators and telescope apertures the whole instrument is

covered by thermal blankets consisting of 22 layers of aluminised Mylar and Kapton

separated by Dacron netting. The outer layer is black conductive Kapton.

To prevent unnecessary heat leak into the structure from electronics units, some of the

detector electronics (VDS LVPS, VDS MEU and GIS MEU) and the MCU are

mounted on a thermally isolated platform above the optics bench where they can

radiate heat through holes in the MLI directly to space.

2. 1 .4 .1 Heaters

The prime operational heaters consist of sixteen thermofoil heaters each controlled by

an AD590 temperature sensor. The prime heaters can consume 24 watts at full power

but are limited to either ¼, ½, ¾ or full power according to the mode of operation of

CDS. The table below shows heater power setting versus mode.

Mode Power setting

ZZ Zero (MCU off)

Standby full

Ready-GIS full

Ready-VDS ½

Ready-Both ½

Page 12 / 50

The redundant operational heaters consist of a separate set of eight thermofoil heaters

controlled by eight temperature sensors selected from the same set that control the

prime heaters. To proved further redundancy these heaters are controlled by the

CDHS although the switching is done by the MCU. The control of these heaters is

described in section 6.

In addition to the operational heaters there is a prime and redundant set of non-

operational heaters powered directly by the spacecraft for use when CDS is powered

off. Either one of these sets of heaters will consume 50 watts when fully powered.

The spacecraft can control the power to a fixed percentage of full power, in

increments of 5%, or it can use the spacecraft controlled thermistor to control to a

fixed temperature.

Tables 2.1.4.1/4 show the position and resistance of each heater.

2. 1 .4 .2 Temperature monitors

There are 32 AD590 temperature monitors distributed on the CDS1 instrument to

monitor the temperature of the structure, optics bench and other critical areas. Sixteen

of these monitors also control the heaters as mentioned above. Table 2.1.4.5 gives the

position and expected temperature range of each temperature monitor.

In addition to the monitors above there is a pair of spacecraft controlled thermistors

mounted on the front bulkhead to record the temperature when CDS is powered off.

Table 2.1.4.1 Prime Operational Heaters

Heater Ohms

( )

Location

OPH00 241 Forebody -Z end +X/-Y

OPH01 241 Forebody -Z end +X/Y

OPH02 241 Forebody -Z end +X/Y

OPH03 241 Forebody -Z end +X/Y

OPH04 653 -Y s/f between +X rad feet, +Y face

OPH05 653 +Y s/f between +X rad feet, -Y face

OPH06 653 Bulkhead 3, top, -Y side, -X face

OPH07 653 Bulkhead 3, top, +Y side, -X face

OPH08 1120 Bulkhead 4, top, -Y side, -X face

OPH09 1120 Bulkhead 4, top, +Y side, -X face

OPH10 1120 -Y s/f bottom of -Z diag, +X face

OPH11 1120 +Y s/f bottom of -Z diag, +X face

OPH12 290 GI optics bench +Z end of -X face

OPH13 560 GI optics bench middle of -X face

OPH14 560 GI optics bench -Z end of -X face

Page 13 / 50

OPH15 560 NI optics bench -X face

Table 2.1.4.2 Redundant Operational Heater

Heater Ohms

( )

Location

ORH00 134 Forebody -Z end +X

ORH01 134 Forebody -Z end -Y

ORH02 134 Forebody -Z end +Y

ORH03 290 GI optics bench +Z end of -X face

ORH04 290 GI optics bench -Z end of -X face

ORH05 560 NI optics bench -X face

ORH06 653 -Ys/f vertical of b/h 3, -Z face

ORH07 653 +Ys/f vertical of b/h 3, -Z face

Table 2.1.4.3 Prime Non-Operational Heaters

Heater Ohms

( )

Location

NPH00 70.9 Forebody -Z end -Y

NPH01 70.9 Forebody -Z end +Y

NPH02 146 GI optics bench +Z end on +Y face

NPH03 146 GI optics bench -Z end on -Y face

NPH04 166 Elect platform -X face -Y/+Z

NPH05 166 Elect platform -X face +Y/+Z

NPH06 166 Elect platform -X face -Y/-Z

NPH07 166 Elect platform -X face +Y/-Z

Table 2.1.4.4 Redundant Non-Operational Heaters

Heater Ohms

( )

Location

NRH00 70.9 Forebody -Z end -Y

NRH01 70.9 Forebody -Z end +Y

NRH02 146 GI optics bench +Z end on +Y face

NRH03 146 GI optics bench -Z end on -Y face

NRH04 166 Elect platform -X face -Y/+Z

Page 14 / 50

NRH05 166 Elect platform -X face +Y/+Z

NRH06 166 Elect platform -X face -Y/-Z

NRH07 166 Elect platform -X face +Y/-Z

Table 2.1.4.5 Flight Temperature Sensor Locations

Sensor Location Application Normal

Temperatu

re Range

FS00 Front bulkhead, +X

u

/-Y

u quadrant Thermal control 18 to 22

FS01 Front bulkhead, +X

u

/+Y

u quadrant Thermal control 18 to 22

FS02 Front bulkhead, -X

u

/-Y

u quadrant Thermal control 18 to 22

FS03 Front bulkhead, -X

u

/+Y

u quadrant Thermal control 18 to 22

FS04 -Y

u sideframe between +X

u radiator feet Thermal control 18 to 22

FS05 +Y

u sideframe between +X

u radiator feet Thermal control 18 to 22

FS06 Bulkhead 3, top, -Y

u side Thermal control 18 to 22

FS07 Bulkhead 3, top, +Y

u side Thermal control 18 to 22

FS08 Bulkhead 4, top, -Y

u side Thermal control 18 to 22

FS09 Bulkhead 4, top, +Y

u side Thermal control 18 to 22

FS10 -Y

u sideframe, bottom of -Z diagonal Thermal control 18 to 22

FS11 +Y

u sideframe, bottom of -Z diagnoal Thermal control 18 to 22

FS12 Optical bench, +Z

u end of GI compartment, -X

u side Thermal control 18 to 22

FS13 Optical bench, middle of GI compartment, -X

u side Thermal control 18 to 22

FS14 Optical bench, -Z

u end of GI compartment, -X

u side Thermal control 18 to 22

FS15 Optical bench, NI compartment, -X

u side Thermal control 18 to 22

FS16 -Y

u radiator between heat straps Housekeeping -25 to -105

FS17 VDS low voltage box, middle of +Z

u face Housekeeping 10 to 20

FS18 Slit motor housing Housekeeping 20 to 25

FS19 Scan motor housing Housekeeping 20 to 25

FS20 -Y

u actuator housing near windings Housekeeping 10 to 30

FS21 +Y

u actuator housing near windings Housekeeping 10 to 30

FS22 MCU heater drive chip Housekeeping 20 to 35

FS23 Bulkhead 3, middle of bottom Housekeeping 18 to 22

FS24 VDS main electronics box, +X

u face under MLI Housekeeping 8 to 16

Page 15 / 50

FS25 GIS main electronics box, +X

u face under MLI Housekeeping 8 to 16

FS26 Electronics platform, -Z

u end between GIS and VDS

boxes

Housekeeping 12 to 23

FS27 MCU electronics box, middle of +Z

u face Housekeeping 12 to 23

FS28 STOP1 near interface with heat strap Housekeeping -10 to +5

FS29 STOP2 at +X

u end of shaft Housekeeping -15 to -5

FS30 Scan mirror housing Housekeeping 15 to 25

FS31 Telescope mount near baffle interface Housekeeping 15 to 25

SC00 Front bulkhead Non-op heaters 15 to 25

SC01 Front bulkhead Non-op heaters 15 to 25

2. 1 .5 Mechanical Design

1. Overall layout, etc, a few diagrams , etc

2. 1 .6 Optical Design

2. 1 .6 .1 General Description

with diagrams

Page 16 / 50

2. 1 .6 .2 Telescope

2. 1 .6 .3 Gratings

2. 1 .6 .4 Scan Mirror

2. 1 .6 .5 Detectors

2. 1 .7 Mechanisms

2. 1 .7 .1 Slit

2. 1 .7 .2 Mirror

2. 1 .7 .3 Offset Pointing System

2. 1 .7 .4 Doors

2. 1 .8 Thermal Control System

2. 1 .8 .1 General Description

2. 1 .8 .2 Heaters

2. 1 .8 .2 .1 Non-op

2. 1 .8 .2 .2 Prime

2. 1 .8 .2 .3 Backup

2. 1 .8 .3 Temperature Sensors

2. 2 CDS Electrical Architecture

2. 2 .1 Electrical block diagram - Alecs Picture

2. 2 .2 Power Switching

2. 2 .3 Redundancy - SCIF, IMIF, Science interfaces, power

2. 3 Operational Concepts

Page 17 / 50

2. 3 .1 CDS Modes

2. 3 .1 .1 ZZZ

2. 3 .1 .2 SBY

2. 3 .1 .3 ESB

2. 3 .1 .4 R-GIS

2. 3 .1 .5 R-VDS

2. 3 .1 .6 R-BOTH

2. 3 .2 Observing Sequences

2. 3 .3 Instrument Health Monitoring

2. 3 .3 .1 Engineering data

2. 3 .3 .2 Housekeeping data

2. 3 .3 .3 On-board health checks

2. 3 .3 .4 EGSE Alarm Concepts

2. 4 CDS Commanding and Control

2. 4 .1 Introduction

2. 4 .2 Types of Command

2. 4 .2 .1 Direct

2. 4 .2 .2 Table load

2. 4 .2 .3 Deferred

2. 4 .3 Commandable Subsystems

brief description of the function (with refence to commands) of:-

2. 4 .3 .1 EPS

Page 18 / 50

2. 4 .3 .2 CDHS (hardware)

2. 4 .3 .3 MCU

2. 4 .3 .4 VDS

2. 4 .3 .5 GIS

2. 4 .3 .6 IMIF Support module

2. 4 .3 .7 MCU Backup module

2. 4 .3 .8 Watchdog module

2. 4 .3 .9 Deferred Command module

2. 4 .3 .10 Macro module

2. 4 .3 .11 Science module

2. 4 .3 .12 Data Compression module

2. 4 .3 .13 Primary memory dump module

2. 4 .3 .14 Secondary memory dump module

2. 4 .3 .15 Two Transputer module

2. 4 .3 .16 Engineering Acquisition module

2. 4 .3 .17 CDHS Internal Telemetry module

2. 4 .3 .18 Health module

2. 4 .4 CDHS Tables

2. 4 .4 .1 Mode Tables

2. 4 .4 .2 Sequence Tables

2. 4 .4 .3 Raster Tables

2. 4 .4 .4 Data Extraction Tables

Page 19 / 50

2. 4 .4 .5 VDS Hardware Tables

2. 4 .4 .6 Solar Event Table

2. 4 .4 .7 Deferred Command Store

2. 4 .5 CDHS Control

3. Instrument Work Station (JP)

3. 1 Configuration

3. 1 .1 What needs to be done (in words)

3. 1 .2 How to do it (which buttons to press etc.)

3. 2 Start Up Procedure

3. 2 .1 W h a t

3. 2 .2 How

3. 3 Commands

3. 3 .1 W h a t

3. 3 .2 How

3. 4 Databases

3. 4 .1 W h a t

3. 4 .2 How

3. 5 Playback

3. 5 .1 W h a t

Page 20 / 50

3. 5 .2 How

3. 6 Data Monitor

3. 6 .1 W h a t

3. 6 .2 How

3. 7 Engineering Monitor (EMON)

The proecdure EMON is provided as a convenient interface to the information

received in the engineering packets of the science telemetry. It can be used

interactively or it can be packaged in its batch mode in other procedures to perform

monitoring tasks on specific groups of parameters.

The use and maintenance of EMON and the associated databases are described in

CDS Software note #26.

3. 7 .1 Daily tasks performed by EMON

It is expected that during the operations day, selected routines based on EMON will be

run on all the telemetry files from the previous day. This will allow monitoring of

critical parameters and maintenance of cumulative use statistics for critical

mechanisms.

Details of the procedures are TBD.

3. 7 .2 What do the Engineering packets in the science stream contain?

There are two kinds of engineering packets in the science stream. They are known as

Engineering A and B. Each contains a different set of parameters. There are various

ways of listing the databases which detail their contents but the easiest, from a non-

specialist user point of view, is to look at the file

$CDS_ENGINEER/new_database.txt

This file gives the parameter names and a brief description.

3. 7 .3 Brief overview of what EMON can be used for.

Details of how to use EMON are given in CDS software note #26.

3. 7 .4 Packaging EMON to perform specific tasks.

Although EMON can work in interactive mode, it can also be packaged to read and

monitor selected parameters in batch mode. One example of this is the routine

EMON_ERROR. This monitors all the parameters in the engineering packets which

may show an error status. Thsi routine is set running and it prints on the screen any

parameter currently showing an error status. Beware however that depending on the

CDS state, an error status on some parameters may not necessarily be a cause for

concern.

Page 21 / 50

3. 7 .4 .1 Packaging EMON to perform specific tasks.

Include existing examples.

3. 7 .4 .2 Error monitoring (EMON_ERROR)

4. Observation Planning (CDP)

4. 1 Overview of planning

Philosophy of planning in view of need for non-RT observations. Resume of how

observations are controlled on board (deferred command list, sequence tables, raster

tables etc.) Resume of how complete planning process is supposed to work.

4. 1 .1 Overview

Apart from two months a year, CDS will be out of ground contact for 16 hours each

day. For that time normal operations must occur and therefore must have been

planned beforehand and the instructions loaded on board during the realtime contact.

CDS has provided software tools in IDL to help observers plan the day’s observations.

All of the details relating to planning are kept in databases, also controlled by IDL

software.

4. 1 .2 On board control.

On board, a specification for an observation is held in ’tables’. The hierarchy of tables

can be viewed as follows:

Data extraction tables - these define which pixels are to be extracted from the detector

data and telemetered to ground. For NIS observations there are also associated VDS

extraction window tables, but these are created automatically, and transparently to the

user. Note that their definition depends not only on the extraction window defined by

the user during planning but upon the hardware readout mode currently in use for the

VDS. This is specified in the state planning database (see section ??)

Raster tables - these define the instrument setup for the observation. Their contents are

fully defined in the document "CDHS Macro Process: Practical Implementation" by

K. al-Janabi but contain such user-definable parameters as the detector, slit number,

data compression scheme, size and number of mirror/slit steps in a scan, exposure

time and a reference to which data extraction table to use.

Series tables - these are created automatically by the Command Preparation Tool

(CPT) and the user has no direct control over them. They form the highest level of on

board tables and contain instructions for pointing the CDS (TBC), readying the

detector and pointers to which rasters to run.

The Deferred Command Store (DCS) on board is also an important planning element.

It contains instructions (time-tagged in UT) to start particular series tables running.

Note that observations already running are aborted if a new observation is started by

an instruction

from the DCS.

Page 22 / 50

4. 1 .3 The ground based planning procedure.

The aim of the planning tools is to take the user requirements and translate them into

instructions that can be loaded directly into the on board stores described above.

Again there is a hierarchy of processes, which from the lowest level up is:

MK_RASTER - A raster is a set of exposures which are taken with a particular

instrument configuration and possibly at different pointing locations, defined by the

mirror and slit positions. At its simplest, a raster definition may reduce to a single

exposure. Mk_raster selects the parameters needed to define a raster, including the

spectral extraction (derived from spectral line lists) to be used.

MK_STUDY - creates studies which are packages of one or more rasters. If

appropriate, pointing information can also be associated with each of the rasters

making up the study at this stage. A study definition may also specify that each raster

is to be repeated a number of times.

MK_PLAN - gives an overview of the complete SOHO planning for

a specified time interval and can call MK_DETAIL (by entering edit mode) to plan in

detail the CDS operations. Previously defined studies are inserted into the time-line in

a variety of ways. Any still undefined pointings are supplied at this stage. The basic

study definition may be repeated at the same or different locations in order to build a

more complete observation.

CPT - takes the information in the detailed planning database (created in

MK_DETAIL) and forms data files whose contents can be loaded into the tables on

board to achieve the required observation. This is a non-interactive process. Details of

how to run it are given in CDS software note #25.

Once CPT has run, the complete set of on board tables and the contents

of the DCS are uplinked by running tw Perl scripts from the TCL command line of the

EGSE (see sections ?? & ??).

4. 2 Planning databases and access to them

Resume of database use (why use them).

Explain distinction between private and project databases. Define controls to be

exercised over each of them.

Resume of routines to interact with them (’show’ routines). Reference to software note

#10

4. 2 .1 Overview of planning databases.

It is anticipated that many CDS observations will be repeated during the mission,

indeed it is planned to run some (eg the Synoptic scans) daily. In order to be able to

reuse previously defined observations it was decided that all definitions (from raster to

general time-line) would be kept in databases controlled by IDL software (see CDS

Software note #10). The contents of these databases will be kept for the duration of

the mission and will ensure that definitions are identified uniquely within the

databases. Not only does this obviate the need for constant reinventing of definitions,

but, since the science FITS files will have the database identifications in their headers,

it will always be possible to trace the exact instrument setup used to acquire a dataset.

Page 23 / 50

The databases have been structured to try and keep repetition of information to a

minimum. For instance the raster database is divided into fundamental raster

parameters and a parameter list which forms variations upon the fundamental raster. A

prime example of a variation parameter is the exposure time, which can be expected

to be vary in an observation much more frequently than the size or number of

mirror/slit steps. Redefining the exposure time of an observation therefore only

involves defining a new variation on a raster rather than a complete new raster.

4. 2 .2 Official versus private databases.

The project will keep a set of protected databases which will form the ’official’ CDS

databases. All users will have read access to these but write access will be restricted.

Users are free to have their own copies of databases in order to be able to build up a

’palette’ for use in their own observation planning. All the planning tools allow use of

either private or official databases. A software tool will be provided by which users

can copy their own definitions into the project databases once they have been vetted

for use on board.

4. 2 .3 Controls over access to the databases.

The official databases will be readable by all users so that they can make use of their

contents when planning their own observations. Write access to the official databases

will be strictly controlled (TBD) and probably only allowed from a single account on

the EOF machines.

4. 2 .4 Accessing database information.

Various IDL routines allow users an overview of the contents of the databases or to

extract more explicit data from them. In general routines called ’(x)show....’ or ’list...’

will give an overview or return general information while routines called ’get_...’ will

extract detailed information.

Use the procedure tftd to see lists of such programs. eg.

IDL> tftd,’show*’

will list the following routines relevant to database information

SHOW_DETAIL - List salient points of details database.

SHOW_LINELIST - To list the contents of the linelist database.

SHOW_RASTER - To summarize the descriptions in the raster databases.

SHOW_SCI_PLAN - List salient points of SOHO science plan database.

SHOW_STRUCT - Display contents and breakdown of an IDL structure.

SHOW_STUDY - To summarize the descriptions in the study databases.

while

IDL> tftd,’get_*’

will list routines to extract specific information (and a whole lot

more!)

4. 3 Technical planning (mk_raster)

Review of what it’s for, what it does.

Mention on-line help.

Reference to software note #24 for user guide.

Page 24 / 50

4. 3 .1 Technical planning routines.

MK_RASTER is the first stage in observation planning. It is called technical planning

because it defines the physical setup of the instrument. Although this is of course

designed with a view to the science that is to be done, the scientific aspects do not

enter directly at this stage. To run mk_raster, simply enter the procedure name in any

IDL session that has access to the CDS IDL directories.

When you are just ’playing’ or developing a raster without wanting necessarily to

interact with any databases, you may make use of the parameter which mk_raster can

take. Thus, for instance, if mk_raster is called with an undefined parameter

IDL> mk_raster, raster

that parameter will be returned, on exit, as a structure which contains a full raster

definition. It need not be complete in the sense that it would not be accepted for

insertion to a database but can be used as a temporary storage for your ideas.

Note that the returned structure also contains a number of tags which are only used

internally by mk_raster. If you call mk_raster with a parameter that is already a valid

structure variable, the details contained within the structure will be loaded into the

mk_raster display on startup. There is, furthermore, an exit mode from mk_raster

which allows the structure to be saved to a file. If that mode is used the file can be

restored (you must use the Yohkoh routine RESTGEN) for further use.

4.3.2 Obtaining help on the use of mk_raster.

CDS software note #24 describes mk_raster but note that the main source of helpful

information is the on-line help. Mk_raster can be switched into a special on-line help

mode wherein help on any of the top-level features can be obtained by accessing

(clicking on) that feature.

4. 4 Science planning

mk_study, why and briefly how to use it.

mk_detail, ditto

mk_plan ditto

Reference to software note #??

4. 4 .1 Overview of science planning.

Science planning is the stage of planning concerned with putting together the

technical aspects (rasters) into a useful package that will perform the observation(s)

required to obtain the data to solve the scientific problem that keeps you awake at

night.

4. 4 .2 Creating study definitions.

The first step is to run MK_STUDY. Use the on-line help to understand the logic of

the program, but a few handy starting tips are:

1) Check under the "File" menu that you are accessing the database (private or

official) that you require. In order to use a private database, the environment variable

ZDBASE_USER must point to a directory containing your databases.

2) Select a raster (and a variation when the associated list appears)

3) ADD it to the study definition

Page 25 / 50

4) Repeat steps (2) and (3) for each raster required in the study. 5) Highlight each

raster in turn in the study definition window and decide and enter the parameters you

want associated with that raster (eg. pointing type (and the position if appropriate) and

number of repeats.

6) Enter all the descriptions necessary for the study (title, science objective etc.)

7) When satisfied with the study definition enter it into the database (under the File

menu).

8) Fix any problems that the database access routines throw back at you.

9) Go to (2)

4. 4 .3 Entering details into the plan timeline.

Mk_plan (which calls mk_detail) is the planning routine that creates a time line for

CDS operations. Again use the online help to understand its logic, but you can get

started by following these instructions.

1) Under the "File" menu, make sure you are accessing the database (private or

official) that you require.

2) Call up a study and its variation. The parameters will be loaded into the screen so

you can confirm you have what you intended.

3) If you want to setup a general science plan for the time period then click on the

’science’ button (bottom left). A single layer time plan will appear. The time interval is

defined by clicking the left mouse button to define the etart time and the right mouse

button to define the end time of the period. If you have entered sufficient header

information (objectives etc) you may click the ADD button to get your selection

entered into the plan.

4) To edit the detailed time line you must be in ’details’ mode, so click on the ’details’

button if not.

5) The start time of the study you are about to enter into the plan can be defined either

by clicking the mouse button in the time line graph or by typing a time in the "Current

time" box.

6) Before entering a study into the plan, decide whether it is to be time-tagged (ie start

at a specific time) or not (ie will start when the previous study finishes). If a study is

not time-tagged and no previous study exists, the new study will start at 00:00 hours

UT.

7) Also before entering a study into the time line, you must decide if multiple pointing

are needed, whether this study is to be repeated more than once and whether the

number of repeats of the last raster in the study is as you want it. This latter parameter,

together with repeats of the study as a whole can be used to manipulate the total

duration of

this plan entry.

8) Enter any pointing positions that are still not defined (ie were

defined as ’deferred at the mk_study stage)

9) If you have both entered a start time, recalled a study and supplied all the auxiliary

information you may now add it to the plan by clicking on the ADD button.

10) Build up the (daily) plan by adding the studies you require.

Page 26 / 50

4. 5 Command preparation (CPT)

Review of use.

Reference to software note #25

4. 5 .1 Command preparation.

The Command Preparation Tool (CPT) is somewhat of a black box for users. It is

fully described in CDS Software note #25. It should only be used by operations staff

(TBC).

In its simplest form it takes only one parameter, the date for which

commands are required. Hence:

IDL> cpt,start=’1996-2-24’

will look up the detailed plan in the database for the 24 hours starting at 1996-2-24

00:00 UT and create the text files with the information needed to be uplinked to the

on board tables.

Note that the following environment variables must be defined:

CDS_CP_CVTFILES

CDS_CP_TTCFILES

CDS_CP_LTBFILES

These specify where the various cpt output files will be stored (they

may be the same directory).

4. 6 Uplinking commands via Perl scripts

---> this should link with other commanding sections.

Once CPT had been run on an appropriate IDL session, it is necessary to uplink both

the tables and the DCS contents. That is achieved by running two Perl scripts from the

TCL command line of the EGSE. The commands to load the tables and the DCF are

respectively:

TCL> cpt/PSLOAD 1996-02-24T00:00:00.000Z

where the parameter is the file name (.LTB) assumed) created by cpt, and

TCL> cpt/DFLOAD 1996-02-24T00:00:00.000Z

where the parameter is the file name (.TTC) assumed) created by cpt

4. 7 4.7 Real time operations

What you can and can’t do

TBD

4. 8 Deferred Commands

4. 8 .1 W h a t

4. 8 .2 How

Page 27 / 50

5. Data processing

5. 1 The science telemetry stream.

The science telemetry is downlinked as a stream of data and normally

received at approximately 10 Kbits/sec, although other rates are possible. In this

stream the data are divided into packets of 306 bytes. Each packet has a time stamp

and an identification byte. The packets may contain science data, engineering data or

on board memory dumps. Users and operations staff can monitor the incoming

telemetry by running the IDL procedure STM (Science Telemetry Monitor). See CDS

Software note #27 for details of that program.

5. 2 The telemetry (TM) files.

The EGSE software which receives the telemetry writes it to telemetry (TM) files. A

new file is written every hour, on the hour. It is possible to have read access to the file

currently being written and this is how STM and other programs access so-called

realtime telemetry. Older TM files can be accessed by STM in its ’replay’ mode

5. 3 The science telemetry monitor (STM)

STM can monitor telemetry data from any IDL session that has read access to the

telemetry files (stored in CDS_TM_DATA). It really is a monitor program since it can

only display the incoming data parameters (raster header information for example) and

display the science data. Very little analysis is possible other than determining some

statistics of the data.

Its use is fully described in CDS Software note #27

5. 4 FITS files

=============================================================

=====

What are they

How to check things are working OK

How to read a FITS file and display data in IDL

Use of QL programs.

Reference to software notes # 3 and 20 for details.

=============================================================

========

5. 4 .1 Contents of FITS files.

The format for the storage and distribution of CDS science data is FITS format.

Details of the exact format to be used are given in CDS Software Note #3

Page 28 / 50

5. 4 .2 Creating FITS files

The FITS files are created by the procedure FITSGEN. The use of this program is for

operations staff only and is described in CDS Software note #23

FITSGEN should be started from an IDL session before telemetry reception starts.

5. 4 .3 Checking contents of FITS files

The operation staff should check that the FITS files are being created correctly by

reading and displaying the data from such a file. Use the IDL procedure QL_MENU

to start up the Quick Look (QL) software. A maunal for that is in CDS Software Note

#20

5. 5 Archives

======================================================

Overview of what they will contain

How will they be created?

How to access them.

Distribution of archive CDS data.

======================================================

See CDS software note #29 (TBC)

======================================================

6. Basic Functions (DJP)

6. 1 Emergency Procedures

6. 2 CDS Switch On and Off

6. 2 .1 Power Configuration

6. 2 .2 CDHS Configuration

6. 3 Power-Up Defaults

6. 3 .1 Default Mode

6. 3 .2 Default CDHS Table contents

6. 3 .3 Default Software Status

6. 4 Thermal Control

Page 29 / 50

6. 4 .1 Non-Operational Heaters (Spacecraft Controlled)

6. 4 .2 Operational Heaters

6. 4 .2 .1 Main Heaters

6. 4 .2 .2 Backup Heaters

6. 5 Modifications to Default Configuration

6. 5 .1 Mode Tables

6. 5 .2 System Sequences

6. 5 .3 Redundant hardware

6. 6 System Preparation for Science Observations

6. 6 .1 Secondary Processor

6. 6 .2 Optional CDHS Software Modules

6. 6 .3 Cleaning Up Telemetry Displays

6. 6 .4 Pointing

6. 6 .5 CDS Physical Pointing

6. 6 .6 Pointing Software

6. 6 .7 Mode Transitions

6. 7 Uploading Observing Sequences

6. 7 .1 Uploads

6. 7 .2 Upload Validation

Page 30 / 50

6. 7 .2 .1 Engineering data

6. 7 .2 .2 Special telemetry

6. 8 Recovery From a Cocked Up Situation

7. Scientific Operations (ERB)

This chapter will detail some of the tasks necessary to perform scientific operations

with CDS. It is assumed that the individual detectors have been comissioned and any

adjustable parameters noted.

7. 1 GIS Operation

The GIS has four XUV detectors which can be independently controlled. Adjustable

parameters for each detector include: High Voltage setting; Look up Table

parameters; Detector Enable/Disable; Stim pulse generator; etc.

The GIS operates by sending a continuous stream of event positions to the CDHS,

where it is histogrammed into a spectrum by the CDHS hardware. Thus the CDHS

controls the integration and exposure times for GIS data. It is important to note that

the GIS continues to send event positions to the CDHS when the CDHS is not taking

GIS exposures; the CDHS just ignores them.

7. 1 .1 Pre-operational Checks

7. 1 .1 .1 Adjustable Voltages incl. HV

7. 1 .1 .1 .1 What

7. 1 .1 .1 .2 How

7. 1 .2 Uploading Tables

7. 1 .2 .1 What

7. 1 .2 .2 How

7. 1 .3 Selecting and Running Observation Sequences

7. 1 .3 .1 What

7. 1 .3 .2 How

Page 31 / 50

7. 1 .4 Complete Example

7. 1 .4 .1 What

7. 1 .4 .2 How

7. 2 VDS Operation

7. 2 .1 Pre-operational Checks

7. 2 .1 .1 Exposure Time Increment

7. 2 .1 .1 .1 What

7. 2 .1 .1 .2 How

7. 2 .1 .2 Adjustable Voltages, inc. HV

7. 2 .1 .2 .1 What

7. 2 .1 .2 .2 How

7. 2 .2 Uploading Tables

7. 2 .2 .1 What

7. 2 .2 .2 How

7. 2 .3 Selecting and Running Observation Sequences

7. 2 .3 .1 What

7. 2 .3 .2 How

7. 2 .4 Complete Example

7. 2 .4 .1 What

7. 2 .4 .2 How

7. 3 Combined Operations

Page 32 / 50

7. 3 .1 Configuration Commands

7. 3 .1 .1 What

7. 3 .1 .2 How

7. 3 .2 Upload and Enable

7. 3 .2 .1 What

7. 3 .2 .2 How

7. 4 CDS Pointing

7. 4 .1 Commands

7. 4 .1 .1 What

7. 4 .1 .2 How

7. 4 .2 Inter-Instrument Data Exchange

7. 4 .2 .1 What

7. 4 .2 .2 How

7. 5 Running and Monitoring Observing Sequences

7. 5 .1 Real-time - with Ground Contact

7. 5 .2 Playback - Out of Ground Contact

7. 6 Recovery from Cocked-Up Situation

7. 6 .1 Panic

7. 6 .2 Fix it - don’t call me !

7. 7 Calibration

Page 33 / 50

7. 7 .1 W h a t

7. 7 .2 How

8. Detailed GIS Procedures (ERB/AAB)

8. 1 Four Types of data

There are two formats of data which can be obtained from the GIS detectors. These

are known as `raw´ and `science´ data.

· R aw data with UV

· Science data with UV

· Raw data with filament

· Science data with filament

8. 1 .1 Raw data with UV

The raw data for a chosen detector is sent on special request via the GIS engineering

stream from the GIS to the CDHS. The CDHS recognises the raw data packets and

sends them as special packets in the science stream. The packets consists of the raw

co-ordinates of events. The form is 16 bit data made up of the two 8-bit signals ( A and

B ) from the detector’s ADCs. In certain locations in each packet of data are a random

selection of values from another ADC which measures the total signal (called PHA

(Pulse Height Analysis data)) from the detector for events. There are 88 PHA values

to about 512 event raw data co-ordinates. It is not possible to associate a PHA value

with any particular event although they are evenly distributed throughout the time

taken to fill the raw packet.

From the raw data one therefore obtains A, B and PHA. A header with the

detector number, the HV set and measured, front face bias, MCP current, LLD

setting and count rates is also included.

The reasons for having this mode of data are:

a) to allow the setting of the High Voltage for each detector such that the PHD

(Pulse Height Distribution) is inside the analogue signal window defined by

the lower and upper level discriminators (LLD and ULD). This is the only way

to get accurate intensity measurements.

b) to allow an appropriate look up table (LUT) to be written for that detector.

c) to allow corrections to be made to the science data for any loss of intensity

in a particular line through the use of a particular set of LUT parameters. The

raw data can be put through any LUT on the ground.

Page 34 / 50

When the GIS is not in raw data mode, one of the GIS engineering parameters

is a PHA value from one of the detectors. The detector can be chosen and the

PHA values gathered over time to create a histogram which should reflect the

PHD during the time the detector was being used. It can also be used to

measure the height of the stim signals. Each detector has two stims. The PHA

value should read close to zero when the detector is not at HV and the stims

are off.

8. 1 .2 Science Data with UV

In this mode, the signals from the ADCs, ( A and B ), are put through a LUT on board.

In the LUT each ( A, B ) co-ordinate is associated with an x- position in the spectrum.

All four detectors are used simultaneously in this mode. The data takes the form of a

histogrammed spectrum, 4 ´ 2048 pixels long. Once on the ground the spectra are put

into FITS form. A header with each file gives exposure time, slit and mirror positions

etc.

The purpose of this mode is to obtain large volumes of data from all four

detectors, simultaneously and fast. There is an overhead of ~20 minutes to

build the LUTs, but once this is done it takes 13 seconds at 10 kbit s - 1 , to

transmit a whole spectrum of 8192 pixels where each pixel contains up to

65536 (16-bit) events. Thus if the dwell time is greater than 13 s all the data

can be telemetered, as long as there is no more than 5000 c s - 1 in any pixel (to

prevent saturation of the 16-bits). For the raw data on the other hand, with 1

GIS engineering packet every two seconds, 1440 events per minute can be

received. To obtain 10,000 events then takes about 7 minutes.

8. 1 .3 Filament Data

Two tungsten filaments are mounted in front of the four detectors in the optics bench.

When a current is put through either of the two filaments, electrons are emitted. The

current is programmable.

The detector front face can be biased to ±12

V. The - 12 V setting is for normal

use with the UV, repelling any background electrons. The +12

V setting may

be used to attract the filament electrons to the detectors. (All detectors are

switched together).

The purpose of the filaments is to provide a repeatable and quick view across

the detector active area. They illuminate the whole of the front face, unlike a

UV spectrum. If the filament setting and detector settings are repeated

identically after periods of use, changes in the detector performance can be

monitored. This assumes the filament output does not change at all.

8. 2 Obtaining the best science data

Figure 1 illustrates the procedure, which must be done for each detector. Start by

setting the LLDs to zero. Then for each detector in turn, point at an area of the Sun

giving typical count rates for the experiment to be done, and change to the appropriate

slit. Then:

Page 35 / 50

1. Set the HV until the ratio of ULD to processed counts, displayed on the EGSE, is

in the ratio 1:10. Care must be taken in taking the detectors up to HV. Safety

checks are included in the GIS software; a HV upper limit˙commanding HV

above this will result in the limit only being reached; a MCP current limit˙if the

current is exceeded the HV will be switched off to this detector. Both limits are

commandable.

2. Take a raw data file of about 10,000 events (200 packets ). Record the name of

the raw data file chosen by the EGSE STM.

3. Use the IDL program read_raw_gis on the raw data file obtained to split the data

into two separate files, one containing the raw data co-ordinates (*.raw), the

other the PHA data (*.pha). It is helpful to name the files with the detector

number, filament number, HV setting and date and time. This program draws a

PHD˙a histogram of the PHA data.

4. Check that the HV setting is appropriate by examining the PHD drawn. If

another drawing is required, plotpha.pro draws the histogram again from the

PHA data file. The data starts at the left hand side of the plot at the LLD. The

ULD is not so obvious though. It is at channel 196 - 204 . Table 1 records the

discriminator levels in terms of electrons and in terms of PHA channels. The

PHD should form a peak at about channel 110 (~4 ´ 10 7 electrons), inside this

window. ( e.g. see figure 2 ). Channel 255 corresponds to 1 ´ 10 8 electrons.

5. If the PHD is satisfactory, take a large raw file of about TBD events (TBD

packets? ) for error analysis and meanwhile analyse (see point 6.) the small raw

data file already taken, for LUT parameters. If the PHD is not satisfactory, repeat

from 2., changing the HV setting by 20

V each time until the PHD is good.

However, look at the later notes on count rate dependent Gain Depression.

Page 36 / 50 æ â å

â å æ

â â

1

:

: :

Anode

A B C

Analogue

A/Sum

B/Sum

Do you

want to write

a new LUT

?

Housekeeping

A/Sum

B/Sum

CDHS

EGSE

R q

à

K, F,

Start, Stop

Zpln, %

Calculate

LUT

LUT

IN

A/Sum

B/Sum OUT

Position in

Spectrum

Science Stream

Fits file

YES

NO

(via Spacecraft, DSN etc.)

RAW DATA

SCIENCE DATA

Figure 1 . Flow diagram to illustrate setting up of detectors for science data

6. Use the program vrawnall.pro to look at the raw data taken with a good HV

setting.

· Plot the raw data in polar co-ordinates. The raw data should form a series of

parallel straight lines; spiral arms.

· Change gain and sum (sometimes called zpln ) settings until the polar plot arms

are as straight as possible.

· Plot in intensity co-ordinates.

· Change k and j until the over-plotted straight lines follow the centre of the data

arms.

· Choose start and stop until the over-plotted lines only follow the data arms˙or

just the part of the spectrum of interest. Selecting part of the spectrum in this way will

invalidate any automatic wavelength calibration, but may be useful for reducing fixed

patterning.

· Choose percent to bound the data in each arm to prevent ghosts (see later). Set

this as high as possible for intensity measurements.

Page 37 / 50

· Output the parameters. The LUT parameters to be uploaded are listed in order.

A check on the LUT and a first view of the spectrum can be obtained by writing a

LUT in IDL using mylut.pro . The raw file can be put through the LUT using

uselut.pro.

Figure 2 . A typical Pulse Height Distribution

showing the peak at channel 120.

Detector 1 Detector 2 Detector 3 Detector 4

Electrons Channe

l

Electrons Channe

ls

Electrons Channe

ls

Electrons Channe

ls

LLD0 1.35 e7 34 1.47 e7 38 1.27 e7 32 1.35 e7 34

LLD1 1.42 e7 36 1.55 e7 40 1.37 e7 35 1.45 e7 37

LLD2 1.65 e7 42 1.78 e7 45 1.60 e7 41 1.70 e7 43

LLD3 1.78 e7 45 1.91 e7 49 1.73 e7 44 1.85 e7 47

LLD4 2.11 e7 54 2.29 e7 58 2.11 e7 54 2.24 e7 57

LLD5 2.34 e7 60 2.54 e7 65 2.29 e7 58 2.44 e7 62

LLD6 3.05 e7 78 3.23 e7 82 3.00 e7 76 3.15 e7 80

LLD7 3.30 e7 84 3.56 e7 91 3.20 e7 82 3.43 e7 87

Page 38 / 50

ULD 7.70 e7 196 8.00 e7 204 8.00 e7 204 7.75 e7 198

Table 1 . Calibration points of lower and upper level discriminators.

Repeat 1. - 6. for all four detectors. Then:

7. Upload the LUT parameters to the spacecraft and start to rebuild˙one detector

at a time because the parameters are shared.

8. Now science data may be collected, keeping the HV settings the same as the

reference raw files.

Figure 3 . Showing a raw data file fitted to LUT parameters

8. 3 Pre-processing corrections to the FITs science data

8. 3 .1 Electronic Dead times

There are two electronic dead times. One is associated with the analogue electronics

for each detector standing alone. The other is associated with combining the data from

the four detectors into one stream and the limited rate of data flow to the CDHS.

Page 39 / 50

After the arrival and detection of a photon there follows a finite time before a

new event can be detected, within which any new events will be discarded by

the electronics pile up discrimination. This limits the rate at which events may

be detected and results in a non-linear relationship between the input and

output count rates. The reduction of the global count rate of the detector can

be calculated and therefore compensated for. Provided there is no rapid change

in the input image, this dead time does not alter the distribution of detected

events in the output image. Every `pixel´ is available to detect a new photon

within the same time period˙the length of the period is reduced by dead time

by the same amount for each pixel. i.e. the detection of a photon depends only

on its arrival time, not on its position. The theoretical output rate follows the

law:

( )

R R e

o i

R T

i d = -

. .

where R

i is the input rate, R

o is the output rate and T

d is the dead time, which is

2.6 μs. This relationship is plotted in figure 4 .

In fact the count rate is limited ultimately, by the rate at which information can

be sent to the CDHS from the GIS box, which is 8.9 ´ 10 4 c s - 1 . A FIFO buffer,

512 events deep, is used to store bursts of events closer together, allowing

short bursts of events at a higher count rate. At total (sum of all four detectors)

count rates near to this value it may be possible to reduce the number of

detectors being used. If the count rate from just one detector is still too high,

the intensities must be treated with caution. Very short exposure times could

be used.

The events from the four detectors are combined into one stream on a first

come first served basis. The detector to detector dead time is 600 ns. This

method of choosing the events results in a global deadtime but, as with the

analogue deadtime, does not affect the distribution of events.

Page 40 / 50

Figure 4 . Plot of relationship between output and input count rates

The dead time used in the plot is 2.6 μs. The curve rolls over at higher count rates

leading to a reduction in output count rate at very high input count rates.

Unlike the electronic dead times, all the rest of the corrections need to be applied on a

pixel by pixel basis.

8. 3 .2 Gain Depression

8. 3 .2 .1 Long Term Gain Depression (LTGD)

The cause of this is simply usage of the MCP (see science note by RAH on 4th Feb.

1994). As charge is removed from the MCP channels, the gain is gradually reduced.

This has the effect of reducing the apparent intensity of the line if the high voltage is

not increased to compensate. For GIS, the parts of the detectors illuminated by bright

lines will suffer first. Because of the wide range of intensities being viewed, it will not

be possible to compensate for the LTGD in all lines at once by increasing the high

voltage. A particularly intense line may cause gain depression in neighbouring regions

up to a distance of 1 mm (2% of spectrum).

There are two problems here. One is the global decay of gain across the whole

detector˙caused by outgassing, plate ageing, filament useage etc. The other is

differential decay caused by the fact that the spectrum is always illuminating

the same parts of the detector. I would therefore suggest a two pronged attack.

Page 41 / 50

Firstly, to monitor global decay by using repeated quiet sun measurements,

background count rates or continuum. If quiet regions of the sun are

considered to be stable, then any decrease in intensity can be monitored with

regular viewing of quiet sun regions.

Secondly, to monitor differential decay both by using the quiet sun and the

filaments. A sequence has been suggested which uses a wide slit to view the

quiet sun. Differential decay should show up as dips in the slit image intensity.

The filament electrons illuminate the whole detector surface. Any regions

suffering from gain depression will appear as a region of lower count rate.

As there are four detectors and two filaments, it is better to set up a filament

with one detector at a time. Choose the filament which gives the flattest

spectrum for the detector. In the FM TV test detectors 1 and 4 gave flattest

spectrum with filament 2, and detectors 2 and 3 with filament 1. Take care to

start with a low current and work upwards. Very high count rates can be

obtained very easily and this may not be obvious with the counters limiting at

65,000 c s - 1 .

· Choose a HV setting as before (§ Error! Reference source not found. item 1.)

and put a current through the filament until an event rate of about 5,000 c s

- 1 is

obtained ( or until the correct count rate in non-bright-line regions is obtained˙

see below). The HV and filament current may need to be iterated until a suitable

count rate and PHD is obtained.

· Take raw data and fit a LUT and then take a science data file of filament events.

For a statistically significant histogram to the 5% level, it is necessary to take a

data file with at least 400 events per pixel. (N.B. This is not necessarily the same

as 800,000 counts in total in the event of a not very flat distribution.)

· Take a filament file for every detector regularly (daily at the beginning of the

mission). Correct each histogram by dividing by the exposure time. Then divide

the new histogram by the old to create a correction curve. Any low count rate areas

will show up as depressions in the correction curve. It can be divided into the data

to correct for LTGD.

It may be necessary to close the doors while the filament data is being taken,

because there is no blank slit provided.

The problem with using filaments to monitor global decay is that they

probably will not stay constant in time. The best use would be to set up the

filament and the HV to give the same count rate in non-bright-line regions at

all times. Then dividing one spectrum by the other will give values equal to

1.0 in non-bright-line regions, and more than 1.0 where there has been loss of

sensitivity.

8. 3 .2 .2 Count rate Dependent Gain Depression (CDGD)

This gain depression occurs when there is a high count rate such that the MCP cannot

recharge fast enough to provide full gain for every event. The peak of the PHD for the

affected area moves towards the LLD so that the number of events are not counted

accurately.

Page 42 / 50

Use of the PHD obtained from the raw data is limited because this is a mean

PHD over the whole plate. If one bright line dominates, then the mean PHD

may shift to the left. Seeing this, you may be encouraged to increase the high

voltage, to return the PHD to the central position. However, this may be

compromising the accurate intensity measurements of any lower count rate

lines which are also of interest. The increase in voltage may force them over

the ULD. If there is only one line of interest, it may be possible to change the

HV until the intensity of that line is maximised.

An alternative method to changing the HV is to use a correction curve, as in

figure 5 TBD . Problems occur in the regions of the curve which are double

valued. The smallest slit should be used to minimise count rates and hence

confusion.

Figure 5 . Correction curve for CDGD

8. 3 .3 Background

The detector dark count is less than 1 - 2 c s

- 1 per detector. Background due to

scattered light from the telescope may need to be subtracted, particularly for detector

1.

8. 3 .4 Ghosts

Figure 3 shows the fitting of a LUT to a normal raw file. In the case of bright lines,

the events will tend to spread across to the neighbouring arm (usually to the left).

Ghosts of the line will then appear in the wrong part of the spectrum. Because of the

type of distortion, the ghosts will always appear in well defined positions. A program

called ghost.pro will give the possible positions of any ghosts and vice versa. The

ghost intensity can be added to the true line intensity.

If there are distortions in the image which cannot be removed by adjusting the

gain and offset parameters (see point 6. in § Error! Reference source not

found. ) this may also lead to ghosts.

Ghosts

arm 1 arm 2 arm 3 arm 4

Figure 6 . Demonstrating the cause of ghosting from one spiral arm to another.

Page 43 / 50

Here, an event which should be on arm 3 is spreading to give ghosts on arms 2 and 4.

8. 3 .5 LUT corrections

If the percent parameter in the LUT is set to 100%, then the maximum number of

events will be captured in the science data. There will undoubtedly be some ghosts,

because of small distortions in the data. By adding the intensities from all the ghosts

back onto the true lines the true intensity can be obtained. However, problems may

occur when the ghost of one line appears at the true location of another line. In this

case, it may be better to reduce the percent parameter to cut out the possibility of

ghosting.

100%

70%

Figure 7 . The use of percent to minimise ghosts

The disadvantage of this approach is that the intensity in the spectral lines are not

given by the number of events in the received spectrum.

Using Vrawnall.pro correction factors can be obtained for this. The method is to

select the part of the arm containing the line using start and stop. The percentage of

events found within 100%, and also within percent % can then be measured. The ratio

gives the correction factor. These correction factors are very dependent on the shape

and fit of the data. It is for this reason that the reference file and knowledge of LUT

etc. is so important.

Arm_line.pro can be used to work out the position in terms of pixels of a line given in

terms of spiral arms.

8. 3 .6 Intensity Curves

Once all the corrections have been performed to the data, the received spectra can be

compared with the intensity curves obtained using the calibration data.

8. 3 .7 Wavelength Corrections

The best fits are quadratic. There are two reasons for this. One fundamental reason is

that the detectors are flat whereas the spectral axis is a curved Rowland circle, and the

incident light is at a high grazing incidence angle. This leads to a quadratic error, as in

figure 8 .

Page 44 / 50

The second reason is associated with the LUT. The convolution of the charge

cloud with the anode leads to a reduction in spiral radius. The shrinkage is not

proportional to radius. When a spiral is fitted to the output, the result is a spiral

with fewer arms than in the anode design. Because the position of a spectral

line in this polar plane only shifts in radius and not in q , the line may appear to

be on arm 3 rather than arm 5. This results in another quadratic error in the

wavelength calibration, but this time dependent on the amount of shrinkage. It

can easily be calculated if the LUT parameter start is known (figure 9 ).

There is a program (xerrcomb.pro) to calculate the geometrical error for each

detector with the incident angles of the UV light adjusted accordingly. It also

calculates the error due to the LUT and adds the two together.

Figure 8 . Error on wavelength calibration due to the geometry

Page 45 / 50

Figure 9 . Non linearity in wavelength calibration due to LUT (with start = 4.1).

8. 4 Summary of GIS pre-processing algorithms

8. 4 .1 Dead Times

8. 4 .1 .1 Overview:

A correction is made which will compensate for the effects of two types of deadtime:-

a) Analogue deadtime for each detector - 2.6 μs

b) Digital processing deadtime - 10 μs

8. 4 .1 .2 Input:

Raw count rate per detector, c

n

, where n = 1,2,3,4

Science count rate, s

sum

8. 4 .1 .3 Algorithm:

Let analogue throughput be a

n

Let digital throughput be d

Then:

a

n

= fn( c

n

)

d = fn( s

sum

)

Page 46 / 50

8. 4 .1 .4 Output:

5 values: d c

n

8. 4 .2 Ghosting

8. 4 .2 .1 Overview

Because of imperfections in the SPAN pattern and the finite noise width, intense line

features may cause ghost lines in other parts of the spectrum. This algorithm indicates

ghost channels for any given channel number. The user may then use this algorithm in

order to:-

a) Identify counts from a line of interest which have appeared as ghosts, for the

purpose of intensity measurements.

b) Confirm that a weak feature is not the ghost from a strong line.

8. 4 .2 .2 Input:

LUT parameters ( start and stop )

8. 4 .2 .3 Algorithm:

See elsewhere (IDL procedure GHOST.PRO )

8. 4 .2 .4 Output:

Channel IDs as required by user.

8. 4 .3 LUT Correction

8. 4 .3 .1 Overview

If the LUT involves <100% throughput, then a correction must be made to account for

this loss. The loss will not be uniform over the spectrum but will be largest in those

areas of the spiral where the greatest distortions have occured.

8. 4 .3 .2 Inputs

LUT parameters

Raw data

8. 4 .3 .3 Algorithm

TBD

8. 4 .3 .4 Output

Correction factor per channel per detector L

nx

, where x= 1˘2048

Page 47 / 50

8. 4 .4 Count-rate Dependent Gain Depression

8. 4 .4 .1 Overview

Since MCP gain is reduced as the local count rate is increased, the effective

throughput at any part of the spectrum is a function of the local count rate. This

algorithm calculates the effect of this gain depression in terms of throughput per

channel. An approximation is made in which the positional resolution from the

electronic readout is considered small compared with the spectral line width. The user

is provided with a correction curve which relates measured count rate with corrected

rate per channel.

8. 4 .4 .2 Input:

HV settings

CDGD curves developed from e.g. Spectral Atlas (data in curves must be already

corrected for their own t , a

n

, ghosts and L

nx

).

8. 4 .4 .3 Algorithm:

TBD

8. 4 .4 .4 Output:

For each detector, factors R

nx where:

Corrected count rate in x = R

nx

´ m

x where:

m

x

= (measured c/r in x ´ L

nx

+ measured c/r in ghost ´ L

nghost

) ´ t ´ a

n

8. 4 .5 Long Term Gain Depression

8. 4 .5 .1 Overview

MCPs retain a `memory´ of their previous count-rate history. As the detector is

scrubbed then the gain falls with time. The approach taken here is to compare the

most recent flat-field measurement with one made at the start of the mission in order

to determine the present local throughput.

8. 4 .5 .2 Input:

Flat-field at start of mission

Most recent Flat field

8. 4 .5 .3 Algorithm:

Recent flat field / Early flat field - normalised to 1.0 for low rate parts of the

spectrum.

Page 48 / 50

8. 4 .5 .4 Output:

2048 channel spectrum of corrections per detector = D

nx

8. 4 .6 Sensitivity

8. 4 .6 .1 Overview

Regular measurements will be made of the overall sensitivity of the instrument. These

will be phased with the flat field calibrations such that an estimate of this sensitivity

will be made for each such measurement.

8. 4 .6 .2 Input:

Quite Sun science data close in time to the most recent flat field.

8. 4 .6 .3 Algorithm:

Quiet Sun data with corrections applied for deadtimes, ghosts, LUT rejection, count-

rate dependent gain depression and long term gain depression, instrument efficiency.

8. 4 .6 .4 Output:

Factors S

nx

8. 4 .7 Intensity

True flux for detector n at position x :

=(measured c/r at x ´ L

nx

+ measured c/r in ghost ´ L

nghost

) ´ t ´ a

n

´ R

nx

´ D

nx

´ S

nx

9. Detailed VDS Procedures (WTT)

9. 1 What

9. 2 How

10. Engineering Activities (ECS)

10. 1 Mechanism Maintenance

Page 49 / 50

10. 1 .1 W h a t

10. 1 .2 How

10. 2 Mechanism Monitoring

10. 3 Relay Monitoring

10. 4 VDS Exposure Monitoring

10. 5 Thermal Monitoring

10. 6 Thermal Adjustment

10. 7 Contamination Monitoring

QCM readings etc

11. Appendices

11. 1 Command List

11. 1 .1 W h a t

11. 1 .2 How

11. 2 Telemetry Parameters

11. 2 .1 W h a t

11. 2 .2 How

11. 3 And all other IWS databases ...

11. 3 .1 W h a t

Page 50 / 50

11. 3 .2 How

11. 3 .3