6 2/$5 �%

E I S

R_{(89}

,PDJLQJ 6SHFWURPHWHU

User Needs userneed draft 1

Z:\mwt\Projects\Solar-B\EIS\docs\sys\eng\userneed1d.doc 3 pages

Issue 1 (draft) Document ID EIS-sys-eng-userneed-1 Document File Z:\mwt\Projects\Solar-B\EIS\docs\sys\eng\userneed1d.doc Authors Matthew Whyndham, MSSL VØronique Gorel, UCL/MSSL Date 07/08/98

Contents Introduction...................................................................................................................................... 2 User Needs....................................................................................................................................... 3

6 2/$5 �%

E I S R User Needs

2 / 3

Introduction

This document is part of the framework for systems engineering for EIS. This is described fully in the

Management Plan (ref). In this framework, the development of the system (the EIS instrument) is controlled at the highest level by three documents, namely theUser Needs document, the System Requirements document and the System Specifications document.

The User Needs document (this document) expresses the goals which the system�s operation will achieve.

The System Requirements document (ref) is a Functional Requirements Document. It reflects a subset of the needs by stating the functional requirements of the system and measurable terms (what the system must do).

The System Specification document describes how the system will meet the requirements. This will refer to the technology to be employed (whereas the Requirements do not).

System Requirements

-sys-eng-sysreq User Needs

-sys-eng-userneed

System Specifications

(Solution B)

-sys-eng-Bspecs

System Specifications

(Solution A)

-sys-eng-Aspecs

System Engineering

Management Plan

-sys-eng-manplan

6 2/$5 �%

E I S R User Needs

3 / 3

User Needs

For the purposes of this document the PI plus the Science Team are regarded as the Users of EIS.

The stated needs are as follows :

• Obtain (spatially resolved) spectra of solar plasmas with:

• Strong emission lines in 104 - 107 K range of temperatures, corresponding to transition region, solar flares, corona • several pairs of lines suitable for density diagnostics • good temperature discrimination for flares • lines which permit to see the connectivity ofcoronal plasma to transition regions • Low, intermediate and high FIP lines for abundance measurements.

• Obtain context images of those plasmas.

• Detect features with spatial resolution of (range) 1-2� (arc sec). 2 is required, 1 would be good.

• Measure (spatially resolved) plasma velocity (Doppler shift and Turbulent broadening), for events which have typically velocities from 10 km/s to few 100 km/s.

• All instruments on Solar-B should yield correlated observations, which implies knowledge of the alignment and that the fields of view must overlap; andsynchronised or well time-tagged observations. There is also a need to correlate Solar-B observations with other instruments on ground based or space based observatories.

• Carry out high cadence (rate of successive) observations. A cadence of the order of 10 s - 20 s (TBD) is needed to follow dynamically evolving features like jets and bright points.